Laser Cut Instructions:

1. Create a CAD model and export design as a DXF.
2. Import a DXF file into Inkscape and add your own graphic.
3. Cut and engrave the sign using a laser cutter.